MAJOR EQUIPMENT

There is a vast amount of Equipment and Core Facilities at Emory. The following is  non-exclusive list of equipment that is specifically available at the Emory Gnotobiotic Animal Core (EGAC).

Gnotobiotic Semi-Rigid Isolators (Parkbio): The chamber of the gnotobiotic isolator is constructed of polypropylene on five sides. The front panel or window can be either flexible PVC. The chamber of the isolator is 3’ foot wide rigid each with the capacity to house 16 mice cages each. The isolators are versatile and can be used for containment, germ-free and exclusion applications. The isolators have high quality cartridge type HEPA filters on both intake and exhaust air systems that provide top axenic security. The glove sleeve design is very spacious especially in the shoulder area allowing greater freedom of movement making the semi-rigid isolators highly ergonomic. The isolators are durable and made of impact resistant polypropylene construction which doesn't corrode from sterilants.

Tecniplast ISOcageP Bioexclusion System: These are airtight individual mouse cages with high positive pressure that are specifically designed for germ-free, gnotobiotic and bioexclusion studies. The ISO cage system is the latest design for gnotobiotics and germ-free animals because it allows researchers to undertake up to 36 simultaneous gnotobiotic studies, compared to only one study at a time in conventional multi-cage gnotobiotic isolators. Features include strong bioexclusion for animal protection through cage-level HEPA filter, combining the protection of an isolator with the ergonomics and density of an IVC cage for maximum animal safety, and saves space and costs with multiple studies on the same rack.




